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Project Overview
Type of application: New
	Proponent name:
	Mr. Fabio Capponi

	Company:
	5530 Nunavut Inc.


Schedule:
	Start Date:
	2017-06-15

	End Date:
	2017-07-27

	Operation Type:
	Annual


Project Description: 
The Meadowbank Precious Metal Project is located on crown land north of Baker Lake, in the Kivalliq Region of Nunavut. A total of 33 Claims have been staked by the company to date, and the remaining claims are currently being staked. The Project is split up into three Areas (the northern Area A, the Central Area B and Southern Area C). The proposed 2017 exploration activities on the project include prospecting, geochemical sampling, and ground geophysics. Then intent of the 2017 work is to delineate targets for future drilling. As soon as drillhole targets can been identified, the locations will be sent to the appropriate regulatory bodies for approval. The 2017 exploration program is anticipated to commence approximately June 15th and it is anticipated to run for 6 weeks. A small fly camp will be required to support the exploration activities at the project. It is estimated that no more than approximately 2 m3 of water will be required at the fly camp. When drill targets are identified a larger camp and more water use will be required. An amendment to the permits and licences will be submitted to account for the lareger camp and water use. It is anticipated that all personnel, equipment and supplies will be brought to the project area from Baker Lake along the Angico Eagle Meadowbank road and then slung by helicopter to the camp. A request to use the road is currently being drafted to submit to Agnico-Eagle. A helicopter will remain onsite to move personnel around the project. One or two small fuel caches will be required consisting of less than 4,000 litres of fuel at a time. 
Personnel:
	Persons:
	6

	Days:
	42


Project Map
List of all project geometries: 
	ID
	Geometry
	Location Name

	1936
	polygon
	Western_Atllas_Claims_Outline_nad83z14


Planning Regions:
Kitikmeot
Affected Areas and Land Types
Inuit Owned Surface Lands
Municipal
Settlement Area
Keewatin Planning Region
Project Land Use and Authorizations
Project Land Use
Mineral Exploration
Licensing Agencies
INAC
NIRB
NWB
Other Licensing Requirements
Class B Water License
Class A Land Use Permit
Material Use
Equipment
	Type
	Quantity
	Size
	Use

	Helicopter
	1
	Longranger
	Fly personnel around project and sling supplies from road to camp

	Truck
	1
	Small Flatbed
	Weekly replenishment of food/ garbage removal

	Drill
	1
	Helicopter portable
	Diamond Drilling


Fuel Use
	Type
	Container(s)
	Capacity
	UOM
	Use

	Aviation fuel
	19
	205
	Liters
	Helicopter

	Diesel
	19
	205
	Liters
	Heat, fuel for generator and drill

	Propane
	2
	45
	Liters
	fuel for stove, fridge, hot water


Hazardous Material and Chemical Use
	Type
	Container(s)
	Capacity
	UOM
	Use

	Oil
	2
	1
	Liters 
	Generator


Water Consumption
	Daily Amount (m3)
	Retrieval Method
	Retrieval Location

	2
	Water will be extracted from a small lake using an electrically powered submersible pump with a fine screen (<1/4” openings) on the intake to prevent fish entrapments.
	To be decided, wthin Area A B and C


Waste and Impacts
Environmental Impacts
The potential environmental impacts of the 2017 small scale grassroots exploration program are anticipated to be negligible. All garbage produced from the 2017 program will be properly stored and removed to be disposed of in Baker Lake weekly. Camp greywater will be stored and treated in an excavated sump, which will allow for slow infiltration into the soil and will be located at least 31 m away from any waterbody. As the program progresses and expands all activities will be assessed for environmental impact risks and every measure available will be taken to ensure the protection and preservation of the natural environment. Drill sites will be located at least 31 m from any waterbody. All drillhole locations will be submitted to the proper regulating authorities for approval. Recirculation and filtration equipment will be used to minimize the amount of water used in during drilling activities. Any residual drill water will be contained in sumps at least 31 m from any waterbody. Secondary containment will be used for all fuel and chemicals and appropriate spill kits will be located at each fuel cache, drillhole and camp. All exploration activities will be documented and drill sites photographed to comply with environmental due diligence. Environmental training, monitoring, reclamation, and site clearance surveys will be built in to the program budget to ensure adequate resources are being allocated to environmental management. 
Waste Management
	Waste Type
	Quantity Generated
	Treatement Method
	Disposal Method

	Combustible wastes
	negligable to low
	none
	Baker Lake

	Greywater
	2m3/day
	If available, coarse gravel will be placed in the bottom of the sump to provide filtration
	Sump

	Non-Combustible wastes
	negligable to low
	recycle
	Baker Lake

	Sewage (human waste)
	negligable to low
	lime
	latrine pit
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