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MS ROALD AMUNDSEN: Northwest Passage – In the Footsteps of Roald Amundsen, from Kangerlussuaq, Greenland to Nome, Alaska USA, 20 August to 11 September 2019, Voyage AMNWP1911 (149064) 
Proposal Status: Conformity Determination Issued 
· 
Project Overview
Type of application: New
	Proponent name:
	Karin Strand

	Company:
	Hurtigruten AS


Schedule:
	Start Date:
	2019-08-26

	End Date:
	2019-09-02

	Operation Type:
	Annual


Project Description: 
Non-technical Project Proposal Summary MS ROALD AMUNDSEN Northwest Passage - In the Footsteps of Roald Amundsen Kangerlussuaq, Greenland to Nome, Alaska USA 20 August - 11 September 2019 Voyage AMNWP1911 MS ROALD AMUNDSEN is a newly-launched passenger ship owned/operated by Hurtigruten AS of Tromsø, Norway. One cruise through the historic Northwest Passage from East to West is planned to the Qikiqtaaluk and Kitikmeot regions of Nunavut during summer 2019. There will be up to 480 passengers and 170 crew members (including approx. 20 members of the expedition team) plus one contracted Ice Pilot on board. Project duration in Nunavut is 8 days, from 26 August to 02 September. The vessel will clear immigration and customs in Pond Inlet (arriving from Greenland) and clear out in Ulukhaktok, Northwest Territories en route to Alaska. Community visits are planned for Pond Inlet, Gjøa Haven and Cambridge Bay; with a Nunavummiut Beneficiary (Ms. Ashley Cummings from Pangnirtung, NU) hired to serve as Cultural Interpreter/Guest Lecturer as part of the staff team on board. Local services and guides will be employed when visiting communities. Equipment: MS ROALD AMUNDSEN – passenger ship Proposed use: Vessel providing transportation/accommodations Fuel: 550 metric tonnes, marine diesel fuel Storage Methods: Built-in fuel tanks of the vessel Auxiliary tender boats Quantity: 15 (OXE-brand 7.0 Explorer rubber boats equipped with OXE PRO 150 HP diesel outboard engines) Proposed use: Sightseeing tours and to facilitate shore landings Fuel: 50 litres marine diesel fuel (filled from ship’s main tanks) Kayaks Quantity: 12 doubles and 6 singles Activities include sightseeing by ship, auxiliary boat cruising, kayaking excursions and shore landings for activities such as guided interpretive walks, bird and nature-watching and hiking. Activities will follow standard operating procedures and be managed by the Expedition Leader with the assistance of a highly-experienced team of expedition staff. Landings will be of short duration and in coastal areas. Visits will follow AECO guidelines (www.aeco.no), as well as Welcoming Visitors to Nunavut guidelines and the Code of Conduct for Operators in Nunavut as provided by Cruise Nunavut. No structures will be erected (permanent/temporary), including docks or piers to support the proposed tourism activity. Tenderboats will be used for shore landings in wilderness areas. Appropriate arrangements will be made where docks or piers are available for use. Where applicable, permit/license applications will be submitted to the appropriate authorities and permits/licenses carried on board. A detailed operations plan has been compiled to evaluate environmental aspects of the planned activity and to ensure compliance with requirements under Federal and Territorial legislation. Operations have been planned to be fully self-sufficient, with activities managed by experienced personnel and to be within the search and rescue capability of the vessel, including for medical evacuation. An Environmental Impact Statement has been prepared. Alternatives considered were: •Changes to itinerary •Changes to number of guests •Changes to vessel and auxiliary craft used •Changes to activities •Alternative of not proceeding It is anticipated that the environmental impact resulting from the planned activity will be not more than minor or transitory in nature. 
Personnel:
	Persons:
	671

	Days:
	8


Project Map
List of all project geometries: 
	ID
	Geometry
	Location Name

	4965
	polyline
	New project geometry


Planning Regions:
Qikiqtani
Kivalliq
Affected Areas and Land Types
Inuit Owned Surface Lands
Municipal
Settlement Area
North Baffin Planning Region
Project Land Use and Authorizations
Project Land Use
Marine-Based Activities
Marine-Based Activities
Tourism Activities
Licensing Agencies
TC: Equivalency Certificate 
GN-EDT: 0
CH: Archaeology and Paleontology Research Permit, Class I 
CWS: Migratory Bird Sanctuary permit under the Migratory Bird Sanctuary Regulations
QIA: 0
GN-DOE: Wildlife Observation Licence 
NIRB: 0
Other Licensing Requirements
No data found. 
Material Use
Equipment
	Type
	Quantity
	Size
	Use

	MS ROALD AMUNDSEN
	1
	Length overall 140m, Breadth moulded 23.6m Draft 5.3m, GRT 20889
	Vessel providing transportation and accommodation. Vessel is a new build, to be launched in April 2019.

	OXE-brand 7.0 Explorer auxiliary tender boats – equipped with Oxe Pro 150 HP (Marine Diesel Oil) outboard engines
	15
	Capacity of 18 persons excluding the driver.
	Motorized auxiliary vessel providing transport between ship and shore and for small group guided sightseeing.

	Double kayaks 
	12
	TBA
	Guided sightseeing tours

	Single kayaks 
	6
	TBA
	Guide kayaks (to accompany kayakers on sightseeing tours)

	Palfinger type NDTS 3500H -brand Fast Rigid Rescue Boats
	2
	Capacity of 6 persons each.
	Emergency use only (rescue situations).


Fuel Use
	Type
	Container(s)
	Capacity
	UOM
	Use

	Diesel
	[bookmark: _GoBack]2
	550
	Metric Tons
	Low Sulfur Marine Gas Oil - Main tanks of the vessel. Fuel is obtain using a “straw” down into the main diesel/MGO tank of the ship. Built-in fuel tanks of the vessel. The likelihood of a catastrophic puncture of a fuel tank is extremely low. The vessel also has an ice-class of Polar Code Category B, Ice Class PC-6.

	Diesel
	15
	50
	Liters
	Diesel for the Explorer tender boats (Marine Diesel Oil). Stored onboard each Explorer boat. Filled from ship’s main fuel tanks.


Hazardous Material and Chemical Use
	Type
	Container(s)
	Capacity
	UOM
	Use

	No records found.


Water Consumption
	Daily Amount (m3)
	Retrieval Method
	Retrieval Location

	0
	Production on board (reverse osmosis)
	Produced in Engine space – NOTE – vessel will be launched in April 2019 – the daily amount is unknown at time of submission


Waste and Impacts
Environmental Impacts
The predicted environmental impacts of the undertaking is perceived to be not more than minor or transitory. Details, including mitigations measures, are included in the project document: Project Description and Environmental Impact Statement - Northwest Passage - In the Footsteps of Roald Amundsen, from Kangerlussuaq, Greenland to Nome, Alaska USA, 20 August - 11 September 2019, MS ROALD AMUNDSEN. NOTE: The vessel is a new build and won’t be launched until April 2019. The project amounts of waste to be generated are therefore being listed as TBD (to be determined). 
Waste Management
	Waste Type
	Quantity Generated
	Treatement Method
	Disposal Method

	Sewage (human waste)
	TBD
	Disposal as per Canadian legislation
	Treated on board

	Combustible wastes
	TBD
	Depends upon type of Waste. Removed for disposal at certified reception port, e.g. for plastics. Incinerated as per Canadian legislation, e.g. for paper.
	Separated

	Greywater
	TBD
	Disposal as per Canadian legislation
	Treated on board

	Hazardous waste
	TBD
	Again depends upon the type of Waste: Removed for recycling or disposal at certified reception port
	Depends upon type of Waste. Collected/separated if Batteries; Collected/frozen if Medical and Sanitary; or Collected if Fuels and Oil.

	Non-Combustible wastes
	TBD
	Again depends upon the type of Non-Combustible Waste. Might be Removed for disposal at certified reception port (if separated and refrigerated) if Food Waste, Disposed of as per Canadian legislation if Glass, Removed for recycling or disposal at certified reception port if Aluminum, or Removed for disposal at certified reception port if Dry, non-burnable or Ash (24h burning) wastes.
	Depends upon type of Waste. If Food Waste segregated and refrigerated or grained and disposed of according to MARPOL regulations. If Metal, Glass, Aluminum or Dry, Non-burnable or Ash (24h burning), Separated. 



