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May 27, 2005

Dear Stephen:

Thank you for your email detailing the information you are requesting.   Our response is as follows:

-          Provide a history of the site if it has been used in the past.

This site has not been used by Triex Minerals Corporation in the past.

-          Provide the location of and distance to the closest communities.

The Kirwan Lake camp will be located on the west side of Kirwan Lake, within the Mountain Lake claims area.  The Kirwan Lake camp will be located approximately 100km SW of Kugluktuk.

-          Describe how the camp site was selected.

The location of the camp was selected based on the proximity to the claims, Kirwan Lake and the closeness of the community of Kugluktuk for staging and supplies.

-          Provide a list of existing and proposed camp structures and facilities. 

There are currently no camp structures or facilities.  Once the approvals and permits are in place, the camp will be constructed.  It will consist of 4 sleep tents, 1 kitchen tent, 1 dry tent, 1 office tent, 1 storage tent, and toilet facilities.  The tents will all be 14’ x 16’ in dimension, except for the kitchen which will be 14’ x 32’.

-          Describe the source of power for the camp. 

The camp will be powered by an 8 KVA generator.

· Location of water source (s) (show on map). Estimated use.

The source of water for use at the camp will come from Kirwan Lake.  Later on, during the drilling program, water sources will consist of small lakes and ponds that are in proximity to the drill target locations.  These have not been determined at this time but will be forwarded to DIAND once a drill program has been finalized.  In our water licence application, we have requested up to 5 cubic metres/day for domestic use and 15 cubic metres/day for drilling.

-          Describe the characteristics, quantities, treatment, storage, transport, and disposal methods for the following:

o        Sewage;

There will be a latrine sump located at the camp.  Sewage will be buried in the latrine sump.  The sump will be located a minimum of 30 metres from the normal high water mark of any water body.

· Camp grey water;

There will be a sump for grey water.  The sump will be located a minimum of 30 metres from the normal high water mark of any water body.

· Combustible solid waste;

Combustible solid waste will be incinerated in a designated burn barrel.

· Non-combustible solid waste;

Non-combustible solid waste will be shipped back to Kugluktuk for disposal in the local landfill.

· Bulky items/ scrap metal;

Bulky items and scrap metal will be shipped off site for disposal in Kugluktuk and/or shipped down south for disposal.

· Waste oil/ hazardous waste;

Waste oil and hazardous wastes will be shipped back to Kugluktuk for disposal in designated areas and/or shipped down south for disposal in designated disposal centres.

· Empty barrels/ fuel drums; and

Empty barrels will be removed from site and fuel caches on a regular basis.  There will be at least on empty drum at each fuel storage location for use as part of the spill kits.

o        Other.

N/A

-          Fuel: provide the types, quantities (number of containers, type of containers and capacity of containers), method of storage, method of containment, location of storage (show on map) and uses.

Diesel, 40 drums with a capacity of 205 litres each

Gasoline, 1 drum with a capacity of 205 litres

Aviation fuel, 31 drums with a capacity of 205 litres each

Propane, 13, 100 lb tanks

-          Hazardous materials: provide the types, quantities (number of containers, the type of container and capacity of containers), method of storage, method of containment, location of storage (show on map), and uses.

Hazardous materials, including cleaning products will be stored within the storage tent at the camp.  The drill program has not yet been defined and as such, a drilling company has not yet been selected.  Once the drill program is finalized and drilling company has been contracted, MSDS sheets for all products that they will be using will be provided to both DIAND and the Nunavut Water Board.  Once the camp is approved and constructed, a map showing the location of the various buildings will be provided to DIAND and the Nunavut Water Board.

-          What will be done with drill cuttings?

Drill cuttings will be pumped to a sump that will be located a minimum of 30 metres from the normal high water mark of any water body.

· What will be done with the drill water?

Drill water is re-circulated within the drill.  Any water from drilling activities will be pumped to the sump.

-          Provide a list of equipment with dimensions and uses.

Helicopter, Bell 206B.  The helicopter will be used to transport crews for field work.  Once a drill program is established, the helicopter will also be used to move the drill.

Generator, 8 KVA.  The generator will provide electricity to the camp.

Water pump.  The water pump will be used to obtain water for use at the camp.

Drill – to be determined once a drill program is finalized.

-          Describe how and when the following will be transported to the project site: (i.e. overland, helicopter, fixed wing aircraft, snowmobile, ATV, Bombardier, barge, other)

o    Equipment

Equipment will be transported to the camp via twin otter (on floats).  Drill moves will be done using the helicopter.

· Camp

Infrastructure for the camp will be transported via twin otter.

· Fuel

Fuel will be transported to the camp via twin otter.  Fuel caches will be established a minimum of 30 metres from the normal high water mark of all water bodies.

o    Chemicals

Transportation of chemicals will follow the Transportation of Hazardous Goods regulations.  Chemicals will be flown in via twin otter.

· Explosives

There will not be any explosives.

· Personnel

Personnel will arrive via twin otter.  Personnel will be transported for field work via the helicopter.

The camp, all supplies, equipment, fuel and personnel will be transported once all of the applicable permits have been obtained.  The project is currently proposed to begin July 1, 2005.

· Describe the level of public involvement, a summary of public involvement measures.

A meeting was held in Kugluktuk with the KIA and the HTO.  Every effort will be made to hire people locally for any applicable available positions.  Staging for the camp and this project will be from Kugluktuk with available supplies coming from the community.  

If you have any further questions, please do not hesitate to contact Ross McElroy and myself.

Regards,

Allison Rippin Armstrong

Ross McElroy, P. Geol

Senior Geologist

Triex Minerals Corp.
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