Project application #124674
Geotechnical and Environmental Baseline Studies – Pond Inlet Small Craft Harbour Development

	Application Type:
	New

	Project Type:
	Research

	Application Date:
	2016-06-09

	Period of Operation:
	From 2016-07-01 to 2017-09-30

	Proposed Authorization:
	From 2016-07-01 to 2017-09-30


	Project proponent: 
	Marie Cardona
Advisian
600-4321 Still Creek Drive
Burnaby BC V5C6S7
Canada
Tel: 778-945-5205, fax: 



Non-technical project proposal description
	English:
	

	French:
	French not included.

	Inuktitut:
	





Project activities
	Location
	Activity Type
	Land Status
	Site History
	Site Archaeological or Palentological Value
	Proximity to the nearest communities and any protected areas

	General Site Location
	Other
	Municipal
	Reconnaissance investigations in support of the Pond Inlet small craft harbour development have previously been conducted at the site.
	No archaeological/palaeontological historical sites have been found at the site. The study team will abide by any terms and conditions for the protection of archaeological and palaeontological resources provided by the Department of Culture and Heritage.
	The proposed geotechnical and environmental baseline studies will be conducted on land in the community of Pond Inlet and in the marine areas in proximity to the community. The study area encompasses Crown, Municipal, and Commissioner’s Lands.



Project Authorizations
	Authorizing Agency
	Authorization Description
	Current Status
	Date Issued / Applied
	Expiry Date

	Fisheries and Oceans Canada
	Licence to Fish for Scientific Purposes
	Not Yet Applied
	
	

	Nunavut Research Institute
	Registration
	Applied, Decision Pending
	
	

	Indigenous and Northern Affairs Canada
	Class "A" Land Use Permit
	Not Yet Applied
	
	

	Nunavut Water Board
	Authorization or Type "B" Water Licence
	Not Yet Applied
	
	



Community Involvement and Regional Benefits
	Community
	Name
	Organization
	Date Contacted



Equipment to be used (including drills, pumps, aircraft, vehicles etc.):
	Equipment Type
	Quantity
	Size - Dimensions
	Proposed Use

	Drill rig
	1
	Standard - Approx weight 2.5 tons
	Geotechnical studies - Borehole drilling and Cone Penetration Testing

	Support vehicle
	1
	Pick-up truck or equivalent
	Field crew and supplies transport

	Small motorboat
	1
	Standard - approx. length 7.6 metres
	Environmental baseline studies



Detail Fuel and Hazardous Material Use:
	Fuel / Material
	Type
	Number of Containers
	Container Capacity
	Total Amount
	Units
	Proposed Use

	Diesel
	fuel
	1
	100
	100
	Liters
	Fuel for drill rig

	Diesel
	hazardous
	1
	100
	100
	Liters
	Equipment operations

	Hydraulic oil
	hazardous
	1
	5
	5
	Liters
	Equipment maintenance

	Petrol
	hazardous
	1
	50
	50
	Liters
	Drilling

	Anti-freeze
	hazardous
	1
	10
	10
	Liters
	Equipment operations

	Drill grease
	hazardous
	1
	5
	5
	Liters
	Equipment operations

	Sample preservative (in sample bottles)
	hazardous
	1
	1
	1
	Liters
	Sample preservation



Types of Waste Associated with the Proposed Project Activities:
	Project Activity
	Type of Waste
	Projected Amount Generated
	Method of Disposal
	Additional Treatment Procedures

	Other
	Overburden (organic soil, waste material, tailings)
	Five cubic metres
	Spread on seafloor
	N/A

	Other
	Sewage (human waste)
	1 cubic metre
	Portable toilet
	Municipal facility



Project Water Consumption:Description of Existing Environment: Physical EnvironmentDescription of Existing Environment: Biological EnvironmentDescription of Existing Environment: Socioeconomic EnvironmentIdentification of Impacts and Proposed Mitigation MeasuresCumulative Effects
	Daily Amount (m3)
	Proposed Water Retrieval Methods
	Proposed Water Retrieval Location

	2
	Drill water will be sourced from the municipality and/or pumped from the sea
	Location for sourcing water to be confirmed by successful contractor




TABLE 1 - IDENTIFICATION OF ENVIRONMENTAL IMPACTS(P = Positive, N = Negative and non-mitigatable, M = Negative and mitigatable, U = Unknown)
	CONSTRUCTION

	OPERATION

	DECOMMISSIONING


