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[bookmark: _Toc416424797][bookmark: _Toc427155766]Introduction
This Abandonment and Restoration Plan (ARP) applies to mineral exploration activities conducted by 5530 Nunavut Inc. (the “Company”) on the Meadowbank Precious Metal Property (the “Property”), Nunavut, Canada. 
This ARP will come into effect June 1, 2017, pending approval. Copies and updates to this plan may be obtained via the Company or APEX Geoscience Ltd. (“APEX”). The ARP will be replaced, upon approval, if there are any significant changes to the activities outlined in the existing permits which warrant changes to the ARP. Minor changes will be submitted as an addendum to the ARP and submitted to the distribution list as required.
[bookmark: _Toc416424798][bookmark: _Toc427155767]Contact Details
	5530 Nunavut Inc.
	APEX Geoscience Ltd.

	2205-1211 Melville Street
	110-8429-24 Street NW

	Vancouver, BC V6E 0A7
	Edmonton, AB T6P 1L3

	Tel: (778) 389-7274
	Tel: (780) 467-3532

	
	Fax: (780) 467-4025
www.apexgeoscience.com



[bookmark: _Toc416424799][bookmark: _Toc427155768]Purpose and Scope
The purpose of the Meadowbank Precious Metal Property ARP is to provide guidelines to follow during seasonal shutdown and final abandonment of the Property, in order to return exploration sites to as near as possible to natural conditions. 
[bookmark: _Toc416424800][bookmark: _Toc427155769]Other Plans
The ARP should be considered as a part of the property wide management system. Other management plans in place at the Meadowbank Precious Metal Property include:
Emergency Response Plan (ERP)
Environmental Management Plan (EMP)
Fuel Management Plan (FMP)
Spill Prevention and Response Plan (SPRP)
Waste Management Plan (WMP)

[bookmark: _Toc416424801][bookmark: _Toc427155770]Property and Camp Description
The Meadowbank Precious Metal Property is located in the Kivalliq Region of Nunavut, within the 1:250,000 scale NTS map sheets, 66A and 66H. The Property is approximately 30 to 100 km north of the community of Baker Lake. The Property consists of three project areas: Area A to the north, Area B in the centre and Area C to the south (Figure 1 in Appendix 1). 
The proposed exploration program will be supported by a temporary, 6 to 10 person exploration camp. The program is anticipated to commence June 15th, 2017 and run for 6 weeks (42 days). INAC, NWB and NIRB will be notified 30 days prior to the establishment of the camp and fuel cache. Personnel and cargo will be transported to the camp along the Agnico-Eagle Meadowbank Road and then flown to site via helicopter. Structures for the proposed camp may include 4 sleeper tents, 1 kitchen, 1 dry, 1 generator shack, and 1 outhouse. The majority of the structures will be insulated Weatherhaven tents, or similar, with tarp floors (Figure 2 in Appendix 1). 
A fuel cache of less than 4,000 L (approximately 19 drums) will be established on stable ground near the camp, primarily to store diesel and jet fuel. Small quantities of gasoline and propane will also be stored. Small temporary fuel caches (less than 4,000 L), may also be required to supply the drilling and exploration programs. Within 30 days of the establishment of any temporary fuel cache, the appropriate agencies will be notified of the details of the cache including: GPS location, fuel type, container sizes, method of storage and proposed date of removal. The temporary fuel cache GPS locations will also be included in the annual reports submitted to the INAC, NWB and NIRB.
The proposed 2017 exploration activities for the Meadowbank Precious Metal Property include prospecting, till sampling and ground geophysical surveys. The intent of the 2017 exploration program is to delineate targets for diamond drilling. As soon as targets are identified for drilling INAC, NWB and NIRB will be notified and supplied with locations and maps. All exploration work and drilling will be strictly confined to the Areas A, B and C (Figure 1 in Appendix 1).
[bookmark: _Toc416424802][bookmark: _Toc427155771]Schedule
The 2017 exploration program is projected to start June 15 and run for 6 weeks (42 days). Prior to subsequent years program commencements all the regulatory authorities and will be notified and supplied with updated schedules.
As a generalized guide for future timing of activities, equipment and supplies, including camp construction materials, will be mobilized in the spring. It is expected that camp construction will take approximately 1 week. Fieldwork, including mapping, prospecting, geochemical sampling, and ground geophysical surveys can be expected to commence as soon as camp construction begins and run through July and August. Drilling will commence as soon as targets are identified and all equipment can be mobilized, most likely at the beginning of July and may have the potential to continue through the winter. As best as possible, camp location and drilling of targets will be timed appropriately to accommodate for caribou migration and calving timing and areas. 
Exploration programs which include geological mapping, prospecting, geochemical sampling, ground geophysical surveys and drilling are anticipated for 3 to 4 subsequent years, depending on each of the previous year’s results. 
Final abandonment and restoration will commence as soon as possible after it has been determined that the project does not warrant further exploration or following commercial production. The duration of the final abandonment and restoration is dependent on the scale of infrastructure on site and on environmental parameters (physical, biological, and socio economic). All abandonment and restoration work will be completed prior to the date of expiry of any existing or future applicable land use permits and water licenses.
[bookmark: _Toc416424803][bookmark: _Toc427155772][bookmark: _Toc182214770][bookmark: _Toc195437678]Detailed Infrastructure
[bookmark: _Toc416424804][bookmark: _Toc427155773]Proposed Temporary Camp
The following is a list which details the structures, equipment and vehicles that may be constructed or stored at the proposed temporary camp. Prior to construction of a more permeant camp INAC, NWB and NIRB will be notified and an amendment application will be submitted to allow for greater water usage.
[bookmark: _Toc416424805][bookmark: _Toc427155774]Structures
	4
	12’x16’ insulated Weatherhaven tents (or similar) on tarp flooring to serve as sleeper tents and a medical tent

	2
	16’x20’ insulated Weatherhaven tents (or similar) on tarp flooring to serve as a kitchen and dry. The dry will contain 1 sink and 1 shower.

	1
	14’x16’ Weatherhaven tent (or similar) on tarp flooring to serve as housing for a 50kW diesel generator plus backup generator.

	1
	5’x5’ wooden outhouse structures



[bookmark: _Toc416424806][bookmark: _Toc427155775]Other Camp Infrastructure
	2
	Water tanks (1 for kitchen and 1 for dry)

	2
	Water pumps with fish screens and hose line

	1
	Small camp fuel cache, with Insta-Berm (or similar) secondary containment.



[bookmark: _Toc416424807][bookmark: _Toc427155776]Vehicles
	1
	
	Helicopter (A-Star, Bell 407, or longRanger)



[bookmark: _Toc416424808][bookmark: _Toc427155777]Drilling Equipment
	2
	
	Zinex A5 (or similar) diamond drill complete with motor, gear box, drill head, tower, overshot, skids, and housing

	4
	
	Supply pump with shack

	2
	
	Mix tank with pressure pump

	6
	
	Coil heater

	6
	
	Fuel tank

	6
	
	Fly basket for drill equipment, spares, supplies, etc.

	400
	
	3 metre NQ drill rods

	50
	
	NQ casing (various sizes)

	150
	
	100’ hose line



[bookmark: _Toc416424809][bookmark: _Toc427155778]Seasonal Shut downs
[bookmark: _Toc416424810][bookmark: _Toc427155779]Inspection and Documentation
It is anticipated that the temporary fly camp will be completely removed at the end of the 2017 exploration program. If drilling targets are identified on the project a larger and more permeant camp will be required. Prior to a seasonal shutdown of a permeant camp, a complete inspection of all areas will be conducted. Photographs will be taken to document the conditions prior to leaving the site, and will be archived along with photos taken at the beginning of each season. Copies of these photos will be included as part of the Meadowbank Precious Metal Property Annual Report. A copy of the Seasonal Camp Inspection Record is attached in Appendix 2.
[bookmark: _Toc416424811][bookmark: _Toc427155780]Buildings, Content, and Fuel
A full inventory of all structures, equipment, fuel, and other supplies will be taken at the beginning and end of each exploration season. An example of the Camp Inventory Record is attached in Appendix 3.
All food, fuel, wastes, empty fuel drums, and valuable or sensitive equipment will be removed from site. A few wooden structures will be left at the camp. All structures to be left on site will be winterized, closed off, and secured. One structure will be designated to house any chemicals or other hazardous materials that are not suited to outdoor storage. All water tanks and pipes will be drained at the end of each season. Pumps and hoses will be drained and stored inside a secured structure. All mechanical equipment, including vehicles, drill equipment, and generators will be winterized and stored in berms for secondary containment. When possible, the equipment and berms will be fully covered.
All remaining fuel and empty drums will be removed from site. 
[bookmark: _Toc416424812][bookmark: _Toc427155781]Waste
All 2017 wastes will separated into combustible, recyclable or hazardous and backhauled for proper disposal. When a larger and more permanent camp is required the following waste treatments will be used:
Combustible Waste: All combustible waste will be incinerated in accordance with the Nunavut Environmental Guideline for the Burning and Incineration of Solid Waste. Any residual waste (ash) will be placed in sealed containers and backhauled for proper disposal.
Non-Combustible, Recyclable and Hazardous Waste: All non-combustible, recyclable and hazardous wastes will be sealed in appropriate containers and backhauled to Yellowknife for proper disposal.
Grey Water: Camp greywater will be stored and treated in an excavated sump, which will allow for slow infiltration into the soil and will be located at least 31 m away from the high water mark of any water body. If available, coarse gravel will be placed in the bottom of the sump to provide filtration, and supports will be built on the sides to prevent slumping. Filters will be installed on kitchen drains to ensure solid food wastes do not enter the sumps and have the potential to attract wildlife. When full, greywater sumps will be covered with enough material to allow for future ground settlement.
Sewage: Privy pits (outhouses) will be located at least 31 m away from a water body. To control sewage pathogens, outhouses will be periodically treated with lime. When full, the pits will be covered with at least 30 cm of compacted soil.
Contaminated soils/snow: All contaminated soil will be stored in empty 205 liter drums, and will be transported to Yellowknife for proper disposal.
Empty barrels/ fuel drums: Empty drums will be collected and transported to Yellowknife either for disposal at an approved site or for refilling.
For more information on waste generation and management see the Muskox Diamond Property “Waste Management Plan.”
[bookmark: _Toc416424813][bookmark: _Toc427155782]Seasonal Restoration
Any contaminated areas around the camp or drill sites will be treated in accordance with the Meadowbank Precious Metal Property “Spill Prevention and Response Plan.” Any washed out areas will be filled and re-contoured to natural levels. Any areas of disturbed vegetation, including camp, fuel caches or drill sites will be photographed and managed as per recommendation of the INAC inspector. Remediation procedures might include fertilization to encourage re-growth.
[bookmark: _Toc416424814][bookmark: _Toc427155783]Final Abandonment and Restoration
[bookmark: _Toc416424815][bookmark: _Toc427155784]Inspection and Documentation
Prior to final abandonment, a thorough inspection of all areas will be conducted. Any contaminated areas around the camp or drill sites that have gone unnoticed will be treated as per the “Spill Prevention and Response Plan.” Photographs will be taken to include in the final reports submitted to the INAC Inspector and as part of the Annual Report submitted to the INAC, NWB and NIRB. All relevant regulatory agencies will be notified upon final abandonment of the Property.
[bookmark: _Toc416424816][bookmark: _Toc427155785]Buildings, Content, and Fuel
Prior to land use permit, claim or lease termination, all structures, equipment, supplies, and fuel will be removed from the Property with the exception of the drill core stacks, which will be permanently secured on site.
Any wooden floors will be burned in accordance with the Nunavut Environmental Guideline for the Burning and Incineration of Solid Waste, and tent sites may be fertilized, as per recommendation by the Inspector, to encourage re-vegetation. The open burning of structures will only occur after approval from INAC and NWB. A request letter will be submitted to the regulating authorities, which will include the characteristic and volume of material to be burned.
Any materials of value on site will be salvaged.  Local businesses and residents will have the opportunity to salvage any remaining materials that will otherwise be disposed of.
Drills and drilling equipment will be dismantled, packaged, secured, and shipped as per the drill contract. All drill casing will be removed from the ground or cut down to ground level if removal is not possible.
All remaining fuel and empty drums will be removed from site. The soil under and surrounding any area where fuel was stored will be thoroughly inspected for any contamination and photographs will be taken.
[bookmark: _Toc416424817][bookmark: _Toc427155786]Waste
All wastes will be disposed of in accordance with the Meadowbank Precious Metal Property “Waste Management Plan” and any contamination will be treated as per the “Spill Prevention and Response Plan”. Sumps will be inspected to ensure there is no leaching or run-off. Back filling and leveling will be employed as necessary.
[bookmark: _Toc416424818][bookmark: _Toc427155787]Restoration
Tent sites, drill sites, and any other areas disturbed by activities related to exploration at the Muskox Diamond Property will be fertilized as recommended by INAC Inspector to encourage re-vegetation.  Eroded or washed out areas related to exploration activities will be filled and re-contoured to natural levels. Any contaminated areas around the camp or drill sites that have gone unnoticed will be treated as per the “Spill Prevention and Response Plan.”
[bookmark: _Toc416424819][bookmark: _Toc427155788]Post Closure Site Monitoring
After reclamation is complete, annual monitoring may take place. If required, the monitoring may consist of soil and water testing, measuring and documenting plan re-growth, examining potential run-off and erosion problems, and checking the stability and condition of the core boxes. Reports, including photographs, will be submitted to the appropriate regulatory bodies. The monitoring will continue as long as the regulating bodies deem it necessary. 
[bookmark: _Toc416424820][bookmark: _Toc427155789]Emergency Contact Information
[bookmark: _Toc427155790]Table 7.1: Emergency Contact Information
	Contact
	Telephone Number

	Rob L’Heureux, Vice President and Project Supervisor - APEX Geoscience Ltd.
	780-439-5380 (office)
780-916-5482 (mobile)

	Fabio Capponi (5530 Nunavut Inc.)
	(778) 389-7274 (mobile)

	INAC (Nunavut)
	1-800-567-9604

	INAC Manager of Field Operations
	(867) 975-4295 (phone)
(867) 979-6445 (fax)

	Nunavut Water Board
	867-360-6338

	Environment Canada
	867-975-4644
24-hr page: 867-766-3737

	DFO (Central and Arctic Branch)
	519-383-1813

	Government of Nunavut Department of Environment
	867-975-7700 (Iqaluit)







[bookmark: _Toc416424821][bookmark: _Toc427155791]Appendix 1: Figures
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[bookmark: _Toc416424822][bookmark: _Toc427155792]Appendix 2: Seasonal Camp Shutdown Inspection Record
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[bookmark: _Toc416424823][bookmark: _Toc427155793]Appendix 3: Example Camp Inventory Record
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Area

Complete

Comment

Inspector

General Camp area
General camp area inspected for any waste, spills or contamination

General camp area secure for winter

All combustible and non-recyclable waste incinerated

"All non-combustible waste prepared for removal

‘Any unnecessary of excessive vegetation damage

Buildings and Content
Al tents and building complexes secured for the winter and dleared of any debris.

‘Al office equipment; furniture; kitchen equipment recreational equipment and other mobile heavy equipment will be winterised and secured

‘Any equipment not capable of withstanding the harsh winter conditions will be removed

Area inspected for petroleum spills or contamination.

Water Supply System
Water pumps, filtering systems, water lines and any other equipment associated with the water supply system drained and winterised

Water pump shed will be secured.

‘Area inspected for petroleum spills or contamination.

Sewage System
Greywater system drained (ie. no greywater remaining in the discharge pipe).

Greywater sumps treated if required, filed and recontoured

Privy Pits treated with Iye and winterized

Privy Pits secure and cleared of any debris

‘Area inspected for petroleum spills or contamination.

Waste Incinerator
Incinerator Fuel supply shut off using all valves.

incinerator Fuel in appropriate and functional secondary containment adjacent to the incinerator

‘Area inspected for petroleum spills or contamination.

Incinerator area cleared of any debris.

Electrical System
Generator shack and surrounding area inspected for signs of spills and remaining wastes such as oil and grease.

Generator shed islined with enviromat in the event any external spills go unnoticed

Generator drained of fuel and winterized

Generator shack secured for winter

All electrical wires, plugs and sockets which remain in their installed locations are safe and secure

‘All electrical cords temporarily connected to a buildings or machinery unplugged, rolled and stored

Camp Heating Systems
Each 205 L fuel barrel attached to respective tent or building secured and within secondary containment

‘Any remaining fuel in lines will burned out.

Empty propane oylinders ready for transport for refilling or recycling.

ANy sleeping quarters converted to electric heat are secured

Petroleum Products and Storage Facilities
All Fuel stored in appropriate and functional secondary containment

Al Tuel storage areas dearly marked in the event siow dlearing activities are required during spring camp opening

All Fuel storage areas GPS location recorded

Al Tuel labelled properly

“Area inspected for spills or contamination.

Fuel storage area deared of any debris.

Chémicals and Hazardous Waste
All chemicals stored in appropriate building or on within appropriate functional secondary containment

‘All household deaners properly secured and stored in kitchen and dry.

‘All empty bags/containers removed for proper disposal

"Any remaining waste fuel, ol and grease stored in approved and labelled containers for reuse during summer operations.

‘Any hazardous waste that cannot be reused properly stored, sealed, labels, and prepared for removal

‘Area inspected for spills or contamination.

‘Area dleared of any debris

spill Response Kits
spill kitinventory performed

Spill kits not needed over winter relocated to secured building

Spill kits needed over winter (ie. for the remaining petroleum areas) properly stocked and secure

Emergency Response
Fire extinguishersin working order and secure in all necessary locations

Smoke/CO2 detectors in working order and secure in all necessary locations

Fire extinguishers used prepared for removal for refilling

Transportation
Transport areasinduding airstrips, helipads, ATV trails, docks and footpathsinspected for spills or contamination.

Vehicles remaining onsite moved into secure buildings

Vehicles remaining onsite winterized

Drill Sites
Diamond drills disnantled and ready for demobilization or secure in designated storage area

Diamond drills remaining on site winterized

‘Any diill casing unable to be removed flush cut so as to not pose a hazard

Drill sites restored and inspected for any waste, spills of contamination

Drill sites photographed before drilling and after restoration

Documentation
Proper documentation and approvals for allinert and Hazardous waste transport and receiving

Notification to all required authorities of pending seasonal shut down

Baseline samples (ie. water, soil, air quality) collected and all data recorded

Inspections recorded, dated and sgned

Photos taken of camp, drill sites, fuel caches and any other important locafionsitems

Photos of drill lay down storage area

GPS coordinates recorded for camp, fuel storage areas, drill stes, wildlife or habitat sghtings, Archeological/paleontological stesor any areaitems of interes

Descriptions recorded for all wildlife or habitat sghtings, Archeological/ paleontological sites or any area/item of interes!

Year-end inventory of all equipment and buildings left on site

List of all equipment, items and repairsrequired for next operating season
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Seasonal Camp Shut Down Inventory

Container

First Aid Tent

Iltem

First Aid Box 1 - Bandages, Gauze, Pads

Telfa bandages

Quantity

Bag of stick on bandages

Cut to size stick on bandages

Butterfly bandages - size -S,M,L

Triangle bandages

Tensor bandages with padding

Lightweight tensor bandages

Brown tensor bandage for sprains

2x2 gauze

2x2 telfa gauze

4x4 gauze

4x4 telfa gauze

66 gauze

66 telfa gauze

Abd pads

44 Telfa pads

Fye patch

Small burn kit with burn bandages

First Aid Box 2 - Tools

Scissors

Tweezers

Rubber bandage for hemmorage

Magnitying gless for eye injury

Eye wash cup

Wooden tip Qip

Sami splints

Mesh mettle for making splint for hand/arm injury

Fach large and small hockey tape.

Thermometer

Cold paks recycle type

Hot paks crush type instant

Cold paks crush type instant

Set of adjustable collars

Pair disposable gloves - s,myex large

Tongue depressors

Finger tube cage for lacerations

Finger tube gauze

First Aid Box 3 - Other Items

Patient Assessment forms

Bottle of Savon solution

Bottle of Peroxide

Bottles of Saline solution

Epi pen

Stitch kit with surgical needle and thread

Emergency dental kit

Vomit bags

Vomit extractor hand pump

Container

ltem

First Aid Box 4 - Large Items

First Aid Box 5 -

D size oxygen tank

Quantity

E size oxygen tank

H size oxygen tank

Regulator for small tanks

Regulator for larg tanks

Ventalation masks

Plastic Spine Board

Spider Straps for the Spine Board

Head immobilzer for the Spine board

Metal cage basket for the Spine Board

Felt grey blankets

Pillows

Kidney dishes/ bed pans

Needed For Next Season
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Seasonal Camp Shut Down Inventory
Generator Shack
Container Item Quantity Container hem Quantity
Generator shack Box 1 - Large Gear Generator Shack Box 4 -
Generators

Incinerator

Purmp for incinerator
Barel litter

Gas Wobble Pump

Diesel Wobble Puinp

Tie Down Kit for Tidy Tank
Rock saw

Rock saw bladcs

Spade shovels

Square shovels
Cieotaok

Sledge hammers
Oil stoves and elbows
Axes

Tiger torch

Spill kits

Breaker pancls

Generator Shack Box 2 - Small Gear Generator Shack Box 5-
Feet of 3/4" Fuel Line
Feet of 3/8" Fuel Line
Battery Charger
Booster Pack

Ratchet Stiaps

15 Fxtension Cord
Oil Filter Wrench

Large Channel pliers
Fuel Filers
OilFilers

AirFilters

Roll of Absorbent Material

Power Bar

Axe
Pry Bar
Devwalt Corded Diill

Sets of Mastercraft Drill Bits.

Generator Shack Box 3 - Taols Needed For Next Season
Set of Hex Driver Bits

Vise Grips
Pliers

Side Curtters

Channel Pliers

Files (Wood, Metal, Round}

Drivers Bits

Utility Knife
Caulking Gun
TS0 Stapler

Packs of "T 50" 1/4" Staples (5000 cach)
New Dewalt 7 174" Circular Saw Blade

Pair Tin Snips

Stanley 17" Steel Chisel

Rolls of "Petro’ 1hread lape

G Speed Square

Ratchet Set
Tigsavs
Set OF Metric Wrenches

Sct OF Imperial Wrenches
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Seasonal Camp Shut Down Inventory

Kitchen Tent

Container

Item

Kitchen Box 1 - Dishes, Cutlery, Cooking Utensils

Dinner plates, dessert plates, bowls

Quantity

Coffee cups

Juice cups

Forks, spoons, butter knives

Steak knives

Pearing Knives

Cutting knives

Cutlery trays

Serving spoons

Slotted serving spoons

Wooden spoons

plastic spatulas

Whisks

Can openers

Cutting boards

Tongs

Disposable drinking cups.

Tupperware storage containers

Kitchen Box 2 - Cookware, Bakeware

Square cake pans

Round cake pans

Pie pans

Cookie sheets

cake cooling rack

Bread loaf tins

non stickfry pan

Large metal bowls

Small metal bowls

Soup pots with lids

Large pots with lids

Small pots with lids

5 gallon galvonized pot

2 gallon galvonized pot

1 gallon galvonized pot

Sauce pan with lid

Omelet pan with lid

Roasting pans with lids

Kitchen Box 3 - Small_Appllences & Cleaning

Metal sieves

Plastic sieves

Quisenar with grating and slicing blade

Kitchen aide mixer

Coffee Makers

Electric kettle

Toaster

Pump style coffes thermos

Clothes pins

Hand pump for large water bottles

Container

Item

Kitchen Box 4 - Large Kitchen Items

Stand up fridge

uan

Propane stoves

Overhead fans

Grease traps for under sinks

Water cooler

Chest freezers

Barbeque

WMetal brush for B5Q grill

Folding tables

Folding chairs

Plastic bins for holding vegetables

microwave

Floor mats

Kitchen Box 5 - Cleaning

Teatowels

Dishtowels

Rags

Dish racks

Scrub brushes

Rubber gloves

Liquid handsoap.

Smoke/C02 Detectors

Brooms

Dust Pans

Garbage Bins

Wooden Beds

Foamies

Needed For Next Season
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Seasonal Camp Shut Down Inventory
Office Tent
Container Item Quantity Container Item Quantity
Office Box 1 - Safety Gear Office Box 4 {freezables to be sent out for storage)
Safety glasses Epoxy
Ear plugs Enamal paint
Hard hat ear defenders Wet coat tree paint
Safety goggles Marker paint
Dust masks Printer ink
Respirator masks
Respirator filters
Bugrepellant
Bear spray
Plastic rain suites
Mosquito coils
Airhorns
Safety vest
Orange gloves
Leather gloves
Rubber gloves
Coth gloves

Office Box 2 - Field Gear Office Box 5 -
Flagging
Packing tape
Nylon rope
Field books
Rock sample cards
Till sample cards
Core sample cards
Personal FA kits
Sample tags
Sharpies
Cable ties
Security seals
Rope chains
Scale
Electrical power bars
Surge protector
Measuring tape

Office Box 3 - Office Supplies Needed For Next Season
Binders
Stapler
Staples
White board
Dry erase pens
Pens
Pencils
Volt meter
3 hole punch
Push pins
Cameras
Printers
Printer paper
Router stand
Router boaster
Cardless phones
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