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Proposal Status: Closed w/o Conformity Determination 
· Overview
· Documents
Project Overview
Type of application: Amendment
	Proponent name:
	Michael

	Company:
	Aboriginal Affairs and Northern Development Canada


Schedule:
	Start Date:
	2017-01-01

	End Date:
	2019-01-01

	Operation Type:
	Seasonal


Project Description: 
same as intial project description. 
Summary of Modifications: 
The following are two proposed modifications for the Jericho Site Stabilization Project: 1) INAC on behalf of DFO proposes to remove the jetty which is in Carat Lake. The objective of this is to create approximately 1,207 m2 fish habitat of Carat Lake through the development of an underwater rock shoal by excavating the existing causeway to at least 2 meter below normal summer water levels. All infrastructure associated with the water intake jetty will first be removed before excavations will commence. The reclamation of the causeway will be based on Tahera Diamond Corporation’s design plan found in their Closure and Reclamation Plan Update Report (April 2007) which is attached for reference. In the report, the causeway is suggested to be “cut to 2m below the normal summer water level from the northern extent back to a water depth of 3.5m. From 3.5m water depth to 1m the causeway will taper up. The reclaimed causeway will intersect surface near the shoreline.” This work will be conducted between July 1 to Aug 31 so as to not have any adverse impacts on the aquatic ecosystem. To isolate the jetty from the lake during the construction, silt booms and/or silt curtains will be used as sediment and erosion control measures. Additional sediment and erosion control measures that will be considered during in water workings are available on the DFO website at http://www.dfo-mpo.gc.ca/pnwppe/measures-mesures/measures-mesures-eng.html. A qualified biologist or environmental inspector will be on site during all in-water restoration/construction works . 2) As a contingency measure to aid in the removal of the frozen core West Dam, explosives may be used. The details of this can be found in the attached document prepared by Outcome Consultants and Rowes Construction. 
Personnel:
	Persons:
	50

	Days:
	180


Project Map
List of all project geometries: 
	ID
	Geometry
	Location Name

	2773
	point
	Jericho

	2774
	point
	Carat Lake

	2775
	point
	Lake C3

	2776
	point
	Lake C1

	2777
	point
	Lake C2

	2778
	point
	Southeast Lake

	2779
	point
	Ash Lake

	2780
	point
	Key lake

	2781
	point
	Lynne Lake

	2782
	point
	Lake C4

	2783
	point
	C1 Diversion

	2784
	point
	East Sump

	2785
	point
	Airport Shed

	2786
	point
	Terminal Building - Camp

	2787
	point
	Camp Storage Shed

	2788
	point
	Main Camp

	2789
	point
	Process Plant

	2790
	point
	Stockpile Shed

	2791
	point
	Truck Shop Shed

	2792
	point
	Truck Shop

	2793
	point
	Gensets

	2794
	point
	Core Shack

	2795
	point
	Offices

	2796
	point
	Kitchen

	2797
	point
	Recreation

	2798
	point
	Wastewater Treatment

	2799
	point
	Wood Shed

	2800
	point
	Genset

	2801
	point
	Parts Wing

	2802
	point
	Storage/Environment Wing

	2803
	point
	Explosive Magazine Storage

	2804
	point
	Emulsion Plant

	2805
	point
	Hazardous Waste Transfer Area

	2806
	polyline
	Existing Permitted JV Winter Road to Lupin Mine

	2807
	polyline
	Proposed Lupin to Jericho Road Extension

	2808
	point
	Borrow Area A

	2809
	point
	Former Carat Camp Area

	2810
	point
	Core Box Laydown

	2811
	point
	Water Intake Jetty

	2812
	point
	Waste Rock Pile

	2813
	point
	Tank Farm - Phase 2

	2814
	point
	Tank Farm - Phase 1

	2815
	point
	Low Grade Stockpile

	2816
	point
	Airstrip

	2817
	point
	f2017516122253-Infrastructure

	2818
	point
	Lupin Mine


Planning Regions:
Qikiqtani
Affected Areas and Land Types
Inuit Owned Surface Lands
Settlement Area
Project Land Use and Authorizations
Project Land Use
Licensing Agencies
NWB: as per past application
KitIA: as per past application
INAC: As per past land use permit application.
Other Licensing Requirements
No data found. 
Material Use
Equipment
	Type
	Quantity
	Size
	Use

	No records found.
	


Fuel Use
	Type
	Container(s)
	Capacity
	UOM
	Use

	No records found.
	
	


Hazardous Material and Chemical Use
	Type
	Container(s)
	Capacity
	UOM
	Use

	No records found.


Water Consumption
	Daily Amount (m3)
	Retrieval Method
	Retrieval Location

	0
	
	


Waste and Impacts
Environmental Impacts
Waste Management
	Waste Type
	Quantity Generated
	Treatement Method
	Disposal Method

	No data found.
	



