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Project Overview
Type of application: Amendment
	Proponent name:
	David Frenette

	Company:
	Agnico Eagle Mines Ltd.


Schedule:
	Start Date:
	2018-05-04

	End Date:
	2025-05-04

	Operation Type:
	Annual


Project Description: 
The present application has been prepared to obtain the authorizations for exploration activities in proposed areas and also include the installation of an exploration camp in one of these areas. The winter accesses already screened will allow Agnico Eagle to transport material and equipment from the Meliadine Mine and from the Whale Cove community to the exploration sites during the winter, thus reducing the use of helicopters during the exploration season. At this time, a limited quantity of material and equipment is planned to be transported, since these exploration projects are at an initial stage. Winter accesses will be used by tracked tractors (Challenger), passing directly on the ice and snow ensuring soil protection. Snowmobiles could also use these accesses. 
Summary of Modifications: 
The present amendment has been prepared to obtain a land use authorisation to conduct mineral prospection activities and geophysical surveys on the expanded “Snow” mineral property. The exploration activities on the original “Snow” area were already authorized by the NPC decision 148849 and the NIRB decision 17EA068. 
Personnel:
	Persons:
	20

	Days:
	60


Project Map
List of all project geometries: 
	ID
	Geometry
	Location Name

	5107
	polygon
	Mineral properties

	5108
	point
	Camp proposed

	5109
	polygon
	Huckleberry-0001

	5110
	polygon
	Snow expansion


Planning Regions:
Kitikmeot
Affected Areas and Land Types
Inuit Owned Surface Lands
Settlement Area
Keewatin Planning Region
Project Land Use and Authorizations
Project Land Use
Mineral Exploration
Licensing Agencies
NIRB: Screening Decision Report 
INAC: Class A Land Use Permit
KivIA: Land Use Licence III
NWB: Type B Licence 
Other Licensing Requirements
No data found. 
Material Use
Equipment
	Type
	Quantity
	Size
	Use

	Diamond drill
	1
	21500kg
	To obtain rock cores.

	Dozer D6
	1
	21500kg
	To move diamond drill during winter period.

	Rab drill
	1
	1500kg
	To obtain rock samples.

	Tracked tractors (Challenger)
	3
	20000kg
	To transport material and equipment on authorized winter access.

	Helicopter
	2
	1500kg
	To transport material, equipment and workers.

	Plane Otter
	1
	2500kg
	To transport material, equipment and workers.

	Mini excavator
	1
	1100kg
	To obtain soil samples, to do small excavations around camp site.

	Snowmobile
	4
	550kg
	Workers transport.

	ATV
	4
	700kg
	Transport around the camps.

	Zoom Boom
	1
	TBD
	Material/equipment handling.


Fuel Use
	Type
	Container(s)
	Capacity
	UOM
	Use

	Aviation fuel
	200
	205
	Liters
	For helicopter and plane.

	Diesel
	200
	205
	Liters
	Drilling, heating, electricity

	Gasoline
	20
	205
	Liters
	For small motors, ATV, snowmobiles

	Diesel
	10
	600
	Liters
	For drilling.

	Diesel
	10
	6000
	Liters
	For drilling.


Hazardous Material and Chemical Use
	Type
	Container(s)
	Capacity
	UOM
	Use

	Grease
	50
	25
	Liters
	Equipment maintenance.

	Glycol
	5
	1000
	Liters
	Equipment maintenance.


Water Consumption
	Daily Amount (m3)
	Retrieval Method
	Retrieval Location

	299
	By pumping
	Proximal lakes, ponds and rivers


Waste and Impacts
Environmental Impacts
Exploration activities in this area are, at this time, planned to be low scale and generate minimal environmental impacts. With all conditions that will be include in NIRB decision, INAC permit, KIA licence, Nunavut Water Board water licence and Agnico Eagle internal management plans, the potential impacts will be mitigated. 
Waste Management
	Waste Type
	Quantity Generated
	Treatement Method
	Disposal Method

	Combustible wastes
	7 tons
	NA
	Incineration and/or transport

	Greywater
	5m³/day
	NA
	Disposed of in natural depression located at more thatn 31m from water body

	Hazardous waste
	5 tons
	Recycling or safe disposal
	Transport in southern facility

	Sewage (human waste)
	2 tons
	NA
	Incineration or transport in southern facility

	Non-Combustible wastes
	5 tons
	NA
	Transport in southern facility



