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The proposed expedition would take place September 21-30, 2019. The expedition is part of the Geological Hazards in Baffin Bay Activity within the Public Safety Geoscience (PSG) Program of the Geological Survey of Canada, which began in 2012, and is funded by the Crown-Indigenous Relations and Northern Affairs Canada (CIRNAC). To date, the activity has resulted in research expeditions in 2013 (NPC 148842, NIRB 13YN021) and 2018 (NPC 148842, NIRB 13YN021), as well as community engagement meetings in 2013, 2014, 2015, 2016, and 2019. Information collected during this project will help support community and government decisions on use of offshore areas and provide communities with better knowledge for improving public safety. 
The proposed research expedition would take place in Baffin Bay between Qikiqtarjuaq and Pangnirtung. Community visits to Qikiqtarjuaq, Pangnirtung, Iqaluit and Pond Inlet were conducted in early 2019 to show results of research conducted during the last 5 years and to propose more research on geological hazards. 
The major goals of this proposed research for 2019 would be: 
-To investigate the stability of the seabed in fjords near Qikiqtarjuaq and Pangnirtung. New imagery of the seabed shows that submarine landslides have occurred in several locations. Baffin Bay experiences a number of earthquakes which can trigger submarine landslides. Our research will help to determine the risk for a large submarine landslide happening in the future. 
-Coastal lakes may also be investigated for the occurrence of tsunami deposits. Coring and mapping of coastal lakes would allow us to collect evidence of past tsunamis affecting the shoreline, similar to the 2017 Greenland tsunami. In addition, digging in coastal areas may take place using shovels to observe if tsunamis have occurred in the past near the villages.
During this type of expedition, we typically collect seabed sediment samples (2 m long gravity cores), seafloor photographs and video, information about the shape of the seabed, and sub-bottom imaging. These instruments will be the same as those used during the 2013 and 2018 expeditions. We also propose using a drone to map fjord wall landslides, and recovering and installing an instrument called an Acoustic Doppler Current Profiler (ADCP) in Southwind fiord for one year that will record any underwater landslides that occur there. The research would take place onboard the Government of Nunavut vessel Nuliajuk. If this project is accepted, the research ship is available from Sept. 21 to 30. 
Research results will be reported back during community visits after the conclusion of the field season or directly following the cruise and will be made publicly available. Results will also be presented at workshops in the North, at science conferences (ArcticNet) and will result in publications in various scientific journals, reports and plain language documents over the months and years following the project.
[bookmark: _GoBack]ᐱᓕᕆᐊᖅ: ᓄᓇᖓᓂ ᖃᐅᔨᓴᕐᓂᖅ ᓴᓐᓂᕈᑎᐅᑉ ᐃᒪᖓᓂ 
[bookmark: _gjdgxs]ᐋᓕᒃᔅᓵᓐᑐᕋᐃ ᓄᐊᒪᑑ, ᑭᐅᕙᓐ ᑳᒻᐳᓪ ᐊᒻᒪ ᕌᐱ ᐱᓂᐊᑦ, ᓄᓇᒥᐅᑕᓕᕆᔨᒃᑯᑦ ᑲᓇᑕᒥ 

ᐊᐅᓪᓚᓂᐅᔪᒪᔪᖅ ᐊᐅᓪᓚᕐᓂᖃᕋᔭᖅᑐᑦᓯᑎᐱᕆ 21-30, 2019. ᐊᐅᓪᓚᕐᓂᐅᔪᖅ ᐃᓚᒋᔭᖓ ᓄᓇᒦᑦᑐᑦ ᐊᑦᑕᓇᖅᑐᓂᑦ ᓴᓐᓂᕈᑎᐅᑉ ᐃᒪᖓᓂ ᖃᓄᐃᓘᕐᓂᐅᔪᑦ ᐃᓗᐊᓂ ᐃᓄᓐᓂᑦ ᐊᑦᑕᓇᐃᖅᓯᒪᑎᑦᑎᓂᕐᒧᑦ ᓄᓇᒥᑦ ᖃᐅᔨᓴᓂᕐᒧᑦ (PSG) ᐱᓕᕆᐊᖅ ᓄᓇᓂᑦ ᖃᐅᔨᓴᓂᕐᒧᑦ ᑲᓇᑕᒥ, ᐱᒋᐊᓚᐅᖅᓯᒪᔪᖅ 2012. ᐅᓪᓗᒥᒧᑦ ᑎᑭᑦᑐᒍ, ᐱᓕᕆᓂᐅᔪᖅ ᓴᖅᑭᑎᑦᑎᓯᒪᔪᖅ ᖃᐅᔨᓴᓂᕐᒧᑦ ᐊᐅᓪᓚᓂᕐᒧᑦ 2013 ᐊᒻᒪ 2018, ᐊᒻᒪᓗᑦᑕᐅᖅᓄᓇᓕᒻᒥᑦ ᐱᖃᑕᐅᑎᑦᑎᓂᕐᒧᑦ ᑲᑎᒪᓂᐅᔪᑦ ᐊᕐᕌᒍᖏᓐᓂᑦ 2013, 2014, 2015, 2016, ᐊᒻᒪ 2019. ᖃᐅᔨᓴᐅᑎᒥᓃᑦ ᑎᑎᕋᖅᑕᐅᓯᒪᔪᑦ ᓄᐊᑕᐅᔪᑦ ᑕᕝᕙᓂ ᐱᓕᕆᐊᒥᑦ ᐃᑲᔪᕐᓂᐊᖅᑐᖅ ᓄᓇᓕᒻᒧᑦ ᐊᒻᒪ ᒐᕙᒪᒃᑯᓐᓄᑦ ᐃᓱᒪᓕᐅᓂᕐᒧᑦ ᐊᑐᖅᑕᐅᓂᖓᓄᑦ ᐃᒪᐃᓐᓇᕐᒥᑦ ᐊᒻᒪ ᓄᓇᓕᓐᓂᑦ ᖃᐅᔨᒪᑎᑦᑎᓂᖅᓴᐅᓗᑎ ᐱᐅᓯᑎᒋᐊᖅᑕᐅᓂᖓᓄᑦ ᐃᓄᓐᓂᑦ ᐊᑦᑕᓇᐃᖅᓯᒪᑎᑦᑎᓂᕐᒧᑦ. 
ᖃᐅᔨᓴᓂᕐᒧᑦ ᐊᐅᓪᓚᕐᓂᐅᔪᒪᔪᖅ ᓴᓐᓂᕈᑎᐃᑉ ᐃᒪᖓᓂ ᐊᑯᓐᓂᖏᓐᓂ ᕿᑭᕐᑕᖅᔪᐊᖅ ᐊᒻᒪ ᐸᓐᓂᖅᑑᖅ. ᓄᓇᓕᒻᒧᑦ ᐅᐸᑦᑕᐅᓂᐊᖅᑐᑦ ᕿᑭᕐᑕᖅᔪᐊᖅ, ᐸᓐᓂᖅᑑᖅ, ᐃᖃᓗᐃᑦ ᐊᒻᒪ ᒥᑦᑎᒪᑕᓕᒃ ᐅᐸᑦᑕᐅᓚᐅᖅᑐᑦ ᐱᒋᐊᕐᓂᖏᓐᓂᑦ 2019 ᑕᑯᔅᓴᐅᑎᑦᑎᓪᓗᑎ ᖃᓄᐃᓐᓂᕆᔭᖏᓐᓂᑦ ᖃᐅᔨᓴᕐᓂᐅᓯᒪᔪᓄᑦ ᐊᕐᕌᒍᓄᑦ ᑕᓪᓕᒪᓄᑦ ᐊᒻᒪ ᖃᐅᔨᓴᒃᑲᓐᓂᕈᒪᓪᓗᑎ ᓄᓇᖓᓂ ᐊᑦᑕᓇᕈᑎᐅᔪᓂᑦ. 
ᑐᕌᒐᓪᓗᐊᑕᕆᔭᖏᑦ ᖃᐅᔨᓴᕐᓂᐅᔪᒪᔪᒧᑦ 2019 ᐅᑯᐊᖑᒐᔭᖅᑐᑦ: 
-ᖃᐅᔨᓴᕐᓗᒍ ᒪᑭᑕᑦᑎᐊᕐᓂᖓ ᐃᖅᑲᖓ ᑲᖏᖅᑐᓂᑦ ᖃᓂᒋᔭᖏᓐᓂᑦ ᕿᑭᕐᑕᖅᔪᐊᖅ ᐊᒻᒪ ᐸᓐᓂᖅᑑᖅ. ᓄᑖᖅ ᐊᔾᔨᓕᐅᕈᑦ ᐃᖅᑲᖓᓄᑦ ᑕᑯᔅᓴᐅᑎᑦᑎᔪᖅ ᐃᒪᐅᑉ ᐃᖅᑲᖓᓂ ᑎᓲᖃᑦᑕᖅᓯᒪᔪᖅ ᐊᒥᓱᐊᒐᓚᓐᓂᑦ ᑕᕝᕙᓂᔅᓴᐃᓇᐅᖏᑦᑐᖅ. ᓴᓐᓂᕈᑎᐅᑉ ᐃᒪᖓ ᐊᒥᓱᒐᓚᐅᓯᒪᔪᑦ ᓄᓇᐅᑉ ᓴᔪᑉᐱᓚᓐᓂᖓᓂᑦ ᐃᒪᐅᑉ ᐃᖅᑲᖓᓂ ᑎᓲᖅᑎᑦᑎᔪᓐᓇᖅᑐᑦ. ᖃᐅᔨᓴᕐᓂᕆᔭᕗᑦ ᐃᑲᔪᓂᐊᖅᑐᑦ ᓇᓗᓇᐃᕐᓗᒍ ᐊᑦᑕᓇᕈᑎᐅᔪᓐᓇᖅᑐᑦ ᐊᖏᔪᑦ ᐃᒪᐅᑉ ᐃᖅᑲᖓᓂ ᑎᓲᕐᓂᐅᔪᓂᑦ ᓯᕗᓂᔅᓴᒥᑦ. 
-ᐃᒪᖅᐸᓯᒻᒦᑦᑐᑦ ᑕᓰᑦ ᖃᐅᔨᓴᖅᑕᐅᑐᐃᓐᓇᕆᐊᖃᕐᒥᔪᑦ ᐃᒻᒪᕐᔪᐊᓚᐅᖅᓯᒪᓂᖓᓄᑦ. ᐳᑑᕆᓂᖅ ᐊᒻᒪ ᓄᓇᖑᐊᓕᐅᕐᓂᖅ ᐃᒪᖅᐸᒥᒻᒦᑦᑐ ᑕᓯᕐᓂᑦ ᐅᕙᑦᑎᓐᓂ ᓄᐊᑦᑎᑎᑦᑎᔪᓐᓇᓂᐊᖅᑐᖅ ᖃᐅᔨᔭᔅᓴᐅᔪᓂᑦ ᐃᒪᕈᕐᔪᐊᓚᐅᖅᓯᒪᓐᓂᖓᓄᑦ ᐊᑦᑐᖅᑕᐅᔪᒥᑦ ᓄᓇᖓᓂ, ᐊᔾᔨᐸᓗᐊᓂ 2017 ᐊᑯᑭᑦᑐᓂᑦ ᐃᒻᒪᕐᔪᐊᕐᓂᐅᔪᖅ. ᐃᓚᒋᐊᕐᓗᒍ, ᖃᓗᕋᕐᓂᖅ ᐃᒪᖅᐸᓯᒻᒥ ᐱᓕᕆᓂᖃᑐᐃᓐᓇᕆᐊᓖᑦ ᐊᑐᕐᓗᑎ ᖃᓗᕋᐅᑎᓂᑦ ᖃᐅᔨᓴᕐᓗᑎ ᐃᒪᕈᕐᔪᐊᓚᐅᖅᓯᒪᓂᖓᓄᑦ ᐅᐊᑦᑎᐊᕈ ᖃᓂᒋᔭᖏᓐᓂ ᓄᓇᓕᓐᓂᑦ.
ᑕᐃᒪᓐᓇᐅᑦᑐᒥᑦ ᐊᐅᓚᕐᓂᐅᔪᒥᑦ, ᓄᐊᑦᑎᒐᔪᓲᖑᔪᒍᑦ ᐃᖅᑲᖓᓃᑦᑐᓂᑦ ᖃᐅᔨᓴᕋᔅᓴᓂᑦ (2 m ᑕᑭᔪᑦ ᐅᖁᒪᐃᓐᓂᖓᓄᑦ ᐳᑦᑐᑎᑦ), ᐃᖅᑲᖓᓂ ᐊᔾᔨᓕᐅᕆᓂᖅ ᐊᒻᒪ ᑕᕐᕆᔭᓕᐅᕐᓂᖅ, ᑐᑭᓯᒋᐊᕈᑏᑦ ᖃᓄᐃᓕᖓᓂᖓᓄᑦ ᐃᖅᑲᖓ, ᐃᑭᐊᖓᒍᑦ ᐊᔾᔨᓕᐅᕆᓂᖅ. ᑖᒃᑯᐊ ᖃᐅᔨᓴᐅᑏᑦ ᐊᔾᔨᒋᓂᐊᖅᑕᖏᑦ ᐊᑐᖅᑕᐅᓚᐅᖅᑐᑦ 2013 ᐊᒻᒪ 2018 ᐊᐅᓪᓚᕐᓂᐅᔪᒥᑦ. ᖃᖓᑕᓲᖑᐊᕋᓛᒃᑯᑦ ᓄᓇᖑᐊᓕᐅᕈᒪᒻᒥᔪᒍᑦ ᑲᖏᖅᑐᖓ ᐊᕙᓗᖓ ᑎᓲᕐᑐᓂᑦ, ᐊᒻᒪ ᐅᑎᖅᑎᑕᐅᓂᖏᑦ ᐊᒻᒪ ᐋᖅᑭᑦᑕᐅᓂᖏᑦ ᖃᐅᔨᓴᐅᑦ ᑕᐃᔭᐅᔪᖅ ᓂᐱᒃᑯᑦ ᑕᕝᕙᑦᑕᐅᑎᒋ ᖃᐅᔨᓴᐅᑦ (Acoustic Doppler Current Profiler) (ADCP) Southwind ᑲᖏᖅᑐᖓᓂ ᐊᑕᐅᓯᕐᒥᑦ ᐊᕐᕌᒍᒧᑦ ᖃᐅᔨᓴᐃᓂᐊᖅᑐᖅ ᖃᓄᐃᑦᑐᑐᐃᓐᓇᕐᓂᑦ ᐃᒪᐅᑉ ᐃᖅᑲᖓᓂ ᑎᓲᕐᓂᐅᖃᑦᑕᖅᑐᓂᑦ.ᖃᐅᔨᓴᕐᓂᖃᕋᔭᖅᑐᑦ ᐅᒥᐊᕐᔪᐊᒥᑦ ᓄᓇᕗᑦ ᒐᕙᒪᒃᑯᑦ ᐅᒥᐊᕐᔪᐊᖓᑦ ᓄᓕᐊᔪᒃ. ᑖᓐᓇ ᐱᓕᕆᐊᖅ ᐊᖏᖅᑕᐅᒍᓂ, ᖃᐅᔨᓴᓂᕐᒧᑦ ᐅᒥᐊᕐᔪᐊᖅ ᐊᑐᐃᓐᓇᐅᔪᖅ ᐱᒋᐊᖅᑐᓂ ᓯᑎᐱᕆ 21 ᑎᑭᑦᑐᒍ 30. 
ᖃᐅᔨᓴᓂᕐᒧᑦ ᖃᓄᐃᓐᓂᕆᔭᖏᑦ ᑐᓴᖅᑎᑦᑎᒍᑕᐅᓂᐊᖅᑐᑦ ᓄᓇᓕᓐᓄᑦ ᐳᓚᕋᓕᖅᑎᓪᓗᒋᑦ ᐱᔭᕇᓚᐅᖅᑎᓪᓗᒍ ᖃᐅᔨᓴᕐᓂᐅᔪᖅ ᐅᕝᕙᓘᓐᓃᑦ ᐅᒥᐊᕐᔪᐊᑰᕋᑖᖅᑎᓪᓗᒋᑦ ᐊᒻᒪ ᑭᒃᑯᑐᐃᓐᓇᕐᓄᑦ ᐊᑐᐃᓐᓇᐅᑎᑕᐅᔪᑦ. ᖃᓄᐃᓐᓂᕆᔭᖏᑦ ᑕᑯᔅᓴᐅᑎᑕᐅᓂᐊᕐᒥᔪᑦ ᑲᑎᒪᓂᐅᔪᓂᑦ ᐅᑭᐅᑕᖅᑐᒥᑦ, ᖃᐅᔨᓴᖅᑏᑦ ᑲᑎᒪᓂᖏᓐᓄᑦ (ArcticNet) ᐊᒻᒪ ᓴᖅᑭᑎᑦᑎᓂᐊᖅᑐᖅ ᐊᔾᔨᒌᖏᑦᑐᓂᑦ ᖃᐅᔨᓴᓂᕐᒧᑦ ᐅᖃᓕᒫᒐᕐᓂᑦ, ᐅᓂᒃᑳᓂᑦ ᐊᒻᒪ ᐅᖃᓕᒫᒐᓇᖏᑦᑐᓂᑦ ᑎᑎᕋᖅᓯᒪᔪᑦ ᑕᖅᑭᐅᓂᐊᖅᑐᓂᑦ ᐊᒻᒪ ᐊᕐᕌᒍᓂᑦ ᐱᔭᕇᖅᓯᒪᓕᖅᑎᓪᓗᒍ ᐱᓕᕆᐊᖅ.


